[Contents] [Prev] [Next] [Index] [Report an Error]

# Specifying an IPv6 Hop Count Limit

You can specify the maximum number of hops that the router can use in router advertisements and all IPv6 packets.

ipv6 hop-limit

- Use to set the maximum number of hops that the router can use in router advertisements and all IPv6 packets.
- Example
  `
  host1(config)#ipv6 hop-limit 50
  `
- Use the no version to set the hop limit for IPv6 packets to 255 hops and router advertisements to zero (0) hops (or “ unspecified” ).
- See ipv6 hop-limit

[Contents] [Prev] [Next] [Index] [Report an Error]