[Contents] [Prev] [Next] [Index] [Report an Error]

# ip dvmrp route-hog-notification

#### Syntax

[ no ] ip dvmrp route-hog-notification [ limit ]

limit—Number in the range 0–2147483647

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the number of DVMRP routes that the router can record before it generates a system log warning message. The no version restores the default setting, 10,000 routes.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]