[Contents] [Prev] [Next] [Index] [Report an Error]

# tcp resequence-buffers connection-maximum

#### Syntax

[ ip ] tcp resequence-buffers [ vrf vrfName ] connection-maximum connMaxValue

no [ ip ] tcp resequence-buffers [ vrf vrfName ] connection-maximum

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
ip keyword made optional in JUNOSe Release 7.2.0.

#### Description

Defines the maximum number of buffers that connections on the current or specified virtual router can use. Specifying a value of zero (0) turns off the connection maximum. The no version reverts the connection maximum value to its default (10 buffers).

#### Options

- ip—Optional keyword for use with older scripts
- vrfName—Name of the VRF; string of 1–32 alphanumeric characters
- connMaxValue—Maximum number of buffers for each virtual router connection, in the range 1–65535

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]