[Contents] [Prev] [Next] [Index] [Report an Error]

# show bgp ipv6 network

#### Syntax

To display information about a prefix configured for all address families or for a specific address family other than the route-target address family:

show bgp ipv6 [ unicast | multicast | vpnv6 all | vpnv6 vrf vrfName ]
network [ ipv6Prefix ] [ filter ]

To display information about about a prefix configured for the route-target address family:

show bgp ipv6 route-target signaling network [ rtfPrefix ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
route-target signaling keywords and rtMemNlri variable added in JUNOSe Release 9.0.0.
rtMemNlri variable replaced by rtfPrefix variable in JUNOSe Release 9.1.0.

#### Description

Displays information about a potentially originated prefix that was configured with the network command.

#### Options

- unicast—Specifies the IPv6 unicast address family and routing table; the default option
- multicast—Specifies the IPv6 multicast address family and routing table
- vpnv6 all—Specifies the VPN-IPv6 address family and all IPv6 VPN routing and forwarding instances
- vpn6 vrf vrfName—Specifies the VPN-IPv6 address family and only the IPv6 VPN routing and forwarding instance with the name vrfName
- ipv6Prefix—Prefix that defines the IPv6 network that you want to filter
- route-target signaling—Displays information for only the route-target address family
- rtfPrefix—Prefix representing the route-target membership NLRI (RT-MEM-NLRI), in the format asNumber:extendedCommunity/prefixLength (for example, 320:320:524/36) where:
  - asNumber—AS number for origin of route target information, in the range 1–4294967295
  - extendedCommunity—Two-part number in the format number1:number2 that identifies an extended community of VPNs, in the format number1:number2, where:
    - number1—Autonomous system (AS) number, in the range 1–4294967295, or an IP address
    - number2—Unique integer, in the range 1–4294967295; 32 bits if number1 is a 16-bit AS number; 16 bits if number1 is an IP address or a 32-bit AS number
  - prefixLength—Number that specifies the length of the route prefix, in the range 32–96
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]