[Contents] [Prev] [Next] [Index] [Report an Error]

# show atm vc

#### Syntax

show atm vc [ atm interfaceSpecifier ] { [ vpi vpi ] [ category categoryType ]
[ status statusType ] | reserved } [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays a summary of all configured ATM virtual circuits (VCs) and reserved VC ranges.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- vpi—Virtual path identifier
- categoryType—One of the following service categories for which VCs are displayed:
  - cbr
  - nrt-vbr
  - rt-vbr
  - ubr
  - ubr-pc
- statusType—Status of VC to be displayed, up or down
- reserved—Displays only a summary of all reserved VC ranges on the router, including those reserved for use by dynamic ATM 1483 subinterfaces and by MPLS
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]