[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Shared Shapers

#### Purpose

Display information about the configured shared shapers.

The best-effort queue is listed as the first resource for shared shapers that are queue controlled. The best-effort scheduler node is listed as the first resource for shared shapers that are node controlled.

#### Action

To display information about configured shared shapers for a specific interface:

    host1#show qos shared-shaper interface atm 11/0
                                                  shared
                                                  shaping shaping
        interface              resource            rate    rate      other
    ----------------- --------------------------- ------- ------- -----------
    atm-vc ATM11/0.10 A atm-vc node                500000         rate 500000
                        atm-vc queue best-effort
                        atm-vc node  EF
                      A atm-vc queue EF voice              100000
                        atm-vc node  AF
                      A atm-vc queue AF video              200000
    atm-vc ATM11/0.11 A atm-vc node                500000         rate 500000
                        atm-vc queue best-effort
                        atm-vc node  EF
    A atm-vc queue EF voice              100000
                        atm-vc node  AF
                      A atm-vc queue AF video              200000

     Total shared shapers:          2
     Total constituents:            12
     Total shared shaper failovers: 0
     Compound shared shapers are not supported

To display information about configured shared shapers for a specific L2TP session:

    host1#show qos shared-shaper l2tp-session session1

To display information about the interface at the root of the scheduler hierarchy located on the tunnel-service interface or at the same hierarchy for LNS GRE tunnel traffic:

    host1#show qos shared-shaper tunnel-server 6/0

To display information about the shared shapers for an interface set:

    host1#show qos shared-shaper qos-interface-set gigEbusiness

To display information about the shared shapers for an interface superset:

    host1#show qos shared-shaper qos-interface-superset allservices

#### Meaning

Table 41 lists the show qos shared-shaper command output fields.

Table 41: show qos shared-shaper Output Fields

Field Name | Field Description
--- | ---
interface | Type of interface
resource | Traffic resource associated with the logical interface
shared shaping rate | Configured shared-shaping rate in bits per second
shaping rate | Individual shaping rate of a traffic resource in bits per second
other | Actual current shaping rate in bits per second
Total shared shapers | Total number of shared shapers
Total constituents | Total number of resource constituents for all shared shapers
Total number of shared shapers that are disabled (in failover mode) due to lack of resources | Total number of shared shapers that are disabled (in failover mode) due to lack of resources
Compound shared shapers are [not] supported | Indication of whether compound shared shapers are supported; determined by installed hardware

#### Related Topics

- Configuring a Scheduler Hierarchy
- Configuring Simple Shared Shaping
- Configuring Compound Shared Shaping
- Configuring Interface Sets for QoS
- Configuring Interface Supersets for QoS
- show qos shared-shaper command

[Contents] [Prev] [Next] [Index] [Report an Error]