[Contents] [Prev] [Next] [Index] [Report an Error]

## Configuring Multicast Listener Discovery

Hosts use Multicast Listener Discovery (MLD) protocol in IPv6 to report their multicast group memberships to neighboring routers. Similarly, multicast routers, such as the E-series router, use MLD to discover which of their hosts belong to multicast groups.

This chapter describes how to configure MLD on an E-series router; it contains the following sections:

- Overview
- Platform Considerations
- References
- Before You Begin
- Configuring Static and Dynamic MLD Interfaces
- Enabling MLD on an Interface
- Configuring MLD Settings for an Interface
- Specifying Multicast Groups
- Assigning a Multicast Group to an Interface
- Configuring Group Outgoing Interface Mapping
- Configuring SSM Mapping
- Limiting the Number of Accepted MLD Groups
- Including and Excluding Traffic
- Configuring Explicit Host Tracking
- Disabling and Removing MLD
- Monitoring MLD
- MLD Proxy Overview
- Configuring MLD Proxy
- Setting the MLD Proxy Baseline
- Monitoring MLD Proxy

[Contents] [Prev] [Next] [Index] [Report an Error]