[Contents] [Prev] [Next] [Index] [Report an Error]

# frame-relay lmi-n392dce

#### Syntax

frame-relay lmi-n392dce threshold

no frame-relay lmi-n392dce

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the error threshold counter (N392) on a DCE interface. The no version removes current setting and sets the default.

#### Options

- threshold—Positive number in the range 1– 10; number of errors that will place the interface in an operationally down state; default value is 2 errors

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]