[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring the Configuration of the HTTP Local Server

#### Purpose

Display information about the configuration of the HTTP local server.

#### Action

To display information about the HTTP local server:

    host1#show ip http server
      Admin status: enabled
      Access class: not defined
      Listening port: 80
      Same host limit: 3
      Protocol: IPv6

#### Meaning

Table 150 lists the show ip http server command output fields.

Table 150: show ip http server Output Fields

Field Name | Field Description
--- | ---
Admin status | Status of the HTTP local server in the software: enabled or disabled. Enabled implies that the HTTP local server can listen for IPv4 , IPv6, or both IPv4 and IPv6 exception packets.
Access class | Name of a standard IP access list that determines which hosts can log on to the HTTP local server
Listening port | Port that the HTTP local server uses to track requests for connection
Same host limit | Maximum number of connections allowed between one IP address and the HTTP local server
Protocol | Protocols that the HTTP local server is listening for: IPv4, IPv6, or IPv4 and IPv6.

#### Related Topics

- show ip http server

[Contents] [Prev] [Next] [Index] [Report an Error]