[Contents] [Prev] [Next] [Index] [Report an Error]

# ip pim query-interval

#### Syntax

ip pim query-interval queryTime

no ip pim query-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
Profile Configuration mode added in JUNOSe Release 8.2.0.

#### Description

Specifies how often the router sends PIM router query messages from this interface. The no version specifies the default time interval, 30 seconds.

#### Options

- queryTime—Interval in the range 0–210 seconds at which the router sends PIM router query messages from this interface

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]