[Contents] [Prev] [Next] [Index] [Report an Error]

# isis retransmit-throttle-interval

#### Syntax

isis retransmit-throttle-interval milliseconds

no isis retransmit-throttle-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the amount of time between retransmissions of any IS-IS LSPs on a point-to-point interface. The no version restores the default value, 33 milliseconds.

#### Options

- milliseconds—Number of milliseconds in the range 0–65535; the minimum delay between LSP retransmissions on the interface

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]