[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 mld version

#### Syntax

ipv6 mld version { 1 | 2 | passive }

no ipv6 mld version

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the MLD version for the interface. The no version restores the default value, MLDv1.

#### Options

- 1—Sets MLD version 1
- 2—Sets MLD version 2
- passive—Configures a mapped OIF as a passive interface with only multicast-data-forwarding capability

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]