[Contents] [Prev] [Next] [Index] [Report an Error]

# bulkstats collector

#### Syntax

bulkstats collector collectorIndex
[ collect-mode { auto-xfer | on-file-full | manual-xfer } | description descrip |
interval intrvl | max-size maxSize | primary-receiver primRecvIndex |
secondary-receiver secRecvIndex | single-interval ]

no bulkstats collector collectorIndex [ collect-mode | description | interval | max-size
|primary-receiver | secondary-receiver | single-interval ]*

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Creates and configures a collector of bulk statistical data to collect MIB-2 ifTable MIB objects. You can configure up to six collectors. The no version restores the default value for specified options; if no options are specified, the no version deletes the collector.

#### Options

- collectorIndex—Number in the range 1–65535 that identifies the particular data collector
- collect-mode—Specifies one of the following collection modes:
  - auto-xfer—Agent automatically transfers file when interval expires
  - on-file-full—Agent automatically transfers file when it is full
  - manual-xfer—Router or user-initiated transfers; default collection mode
- descrip—Descriptive information to insert into the bulkstats file
- intrvl—Time period in the range 300– 86400 seconds for which the collector transfers data from the router to the receivers; default interval is 360 seconds
- maxSize—Maximum size of the file in the range 10240–20971520 bytes; default file size is 2,621,440 bytes
- primRecvIndex—Number in the range 1–65535 that identifies the primary receiver to which the router transfers the data; by default the primary receiver is cleared
- secRecvIndex—Number in the range 1–65535 that identifies the secondary (backup) receiver to which the router transfers the data; by default the secondary receiver is cleared
- single-interval—Specifies that the collector retrieves the bulk statistics data only once; by default, the collector receives the data periodically
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]