[Contents] [Prev] [Next] [Index] [Report an Error]

# encapsulation bridge1483

#### Syntax

encapsulation bridge1483 [ mac-address macAddress ]

no encapsulation bridge1483

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures bridged Ethernet as the encapsulation method on an interface and optionally assigns a MAC address to the interface. The no version removes bridged Ethernet as the encapsulation method on the interface.

#### Options

- macAddress—User-configured MAC address for the interface. The MAC address format is a dotted triple of four-digit hexadecimal numbers; for example, 0090.1a40.4c7c. Multicast MAC address cannot be configured on bridged Ethernet interfaces.

#### Mode

Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]