[Contents] [Prev] [Next] [Index] [Report an Error]

# Troubleshooting

Use the pppPacket log to diagnose problems on your PPP interfaces. On dynamic PPP interfaces, you can use the ppp log command within the profile, as described in Configuring Dynamic Interfaces.

log severity debug pppPacket

- Use to configure a trace log file for a PPP interface.
- Specify one of the following interface types and an interface specifier. For example, specify slot/port:channel/subchannel for a serial POS PPP interface.
  - serial—Serial interface
  - atm—ATM interface
  - pos—Packet over SONET interface
- You also configure logging to direct the output to a specific destination. For information, see Overview of System Logging.
- Example
  `
  host1(config-if)#log severity debug pppPacket serial 0/0:1/1
  DEBUG 01/01/1970 00:16:58 pppPacket (1000001,*): interface:0/0:1/11/0:1,
  time: 0.00, tx lcp confReq, id = 226, length = 19, mru = 32759,
  authentication = chap MD5,magicNumber = 0x5387f9a2
  DEBUG 01/01/1970 00:16:58 pppPacket (1000001,*): interface: 0/0:1/11/0:1,
  time: 0.01, rx lcp confReq, id = 156, length = 18, mru = 32759,
  magicNumber = 0x2d8eac91, pfc, acfc
  DEBUG 01/01/1970 00:16:58 pppPacket (1000001,*): interface: 0/0:1/11/0:1,
  time: 0.01, tx lcp confAck, id = 156, length = 18, mru = 32759,
  magicNumber = 0x2d8eac91, pfc, acfc
  `
- Use the no version to return the severity changes to their default setting or to the systemwide setting.
- See log severity.

ppp log

- Use to enable PPP packet or state machine logging on any dynamic interface that uses the profile being configured. Specify one of the following keywords:
  - pppPacket—Enables PPP packet logging
  - pppStateMachine—Enables PPP state machine logging
- Example
  `
  host1(config-profile)#ppp log pppPacket
  `

  | Note: This command is equivalent to the log severity debug pppPacket and log severity debug pppStateMachine commands.

- Use the no version to disable packet or state machine logging.
- See ppp log.

[Contents] [Prev] [Next] [Index] [Report an Error]