> - Download PDFs
> - Monitoring the Configuration of QoS Interface Sets
> - Related Topics
> - Configuring Interface Sets for QoS
> - show qos-interface-set

> # Monitoring the Configuration of QoS Interface Sets

> #### Purpose

> Display information about configured interface sets.

> #### Action

> To display information about a specific interface set:

>     host1#show qos-interface-set vlan-set
>     interface                  member member restricted
>        set    parent   port     type  count  interface
>     --------- ------ --------- ------ ------ ----------
>     vlan-set  vlan-ss lag test1 vlan   2        none

> To display detailed information about a specific interface set:

>     host1#show qos-interface-set vlan-set detail
>     interface                   member member restricted
>        set    parent    port     type  count  interface
>     --------- ------- --------- ------ ------ ----------
>     vlan-set  vlan-ss lag test1  vlan    2      none

>     Children:
>       vlan lag test1.1      vlan lag test1.4

> #### Meaning

> Table 1 lists the show qos-interface-set command output fields.

> Table 1: show qos-interface-set Output Fields

> Field Name | Field Description
> --- | ---
> interface set | Name of the interface set
> parent | Name of the interface superset that is the parent of the interface set
> port | Interface that is the parent of the interface superset
> member type | Member-interface type defined for the interface set: vlan ip vlan
> restricted interface | Restricted interface configured for this interface set
> Children | List of interface members associated with the interface superset

> #### Updated: 2009-04-06

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.