[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls statistics label

#### Syntax

[ no ] mpls statistics label { interface interfaceName atm vpi vci | labelValue }

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Enables statistics collection for MPLS in labels. By default, statistics are enabled for in labels depending on the protocol that added the in label to the MPLS forwarding table. Statistics are not stored in NVS. The no version disables statistics collection.

#### Options

- interfaceName—Name of interface for label in interface label space on an ATM AAL5 interface; up to 15 alphanumeric characters
- vpi—Virtual path identifier for a label, a value in the range 0–255
- vci—Virtual circuit identifier for a label, a value in the range 33–65535
- labelValue—Integer identifying a label in the platform label space, a value in the range 16–1048575

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]