[Contents] [Prev] [Next] [Index] [Report an Error]

# show egress-queue events

#### Syntax

show egress-queue events { interface interfaceType interfaceSpecifier |
l2tp session sessionName | tunnel-server interfaceType } [ atmVpi | s-vlanIdValue ]
[ explicit | summary ] [ traffic-class trafficClassName ]
[ event-exceeding eventExceedingNumber
{ committed | conformed | exceeded | forwarded } ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
atmVpi and s-vlanIdValue variables added in JUNOSe Release 7.1.0.

#### Description

Displays events that track the number of times egress queuing rates exceed thresholds you have configured.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- sessionName—Name of the L2TP session
- atmVpi—Virtual path identifier of this PVC; number in the range 0–255
- s-vlanIdValue—S-VLAN ID number in the range 0–4095
- explicit—Displays events for queues only on the specified interface and not for queues stacked above the interface
- summary—Displays the sum of events for the queues bound to interfaces that are stacked above the specified interface
- trafficClassName—Name of a traffic class for which egress queue events are displayed
- eventExceedingNumber—Number of events, in the range 1–1073741824
- committed—Displays queues in which the committed drop count exceeds the eventExceedingNumber
- conformed—Displays queues in which the conformed drop count exceeds the eventExceedingNumber
- exceeded—Displays queues in which the exceeded drop count exceeds the eventExceedingNumber
- forwarded—Displays queues in which the forwarding event count exceeds the eventExceedingNumber
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Monitoring Forwarding and Drop Events on the Egress Queue

[Contents] [Prev] [Next] [Index] [Report an Error]