[Contents] [Prev] [Next] [Index] [Report an Error]

# E120 Router Specifications

Table 14: E120 Router Specifications

Category | Specification
--- | ---
Weight |
Chassis only | 51 lb (23.1kg)
Chassis fully configured | Approximately 107 lb (48.5 kg)
Dimensions |
Chassis only | 11.25 (H) x 17.45 (W) x 25.10 (D) inches; 28.57 x 44.32 x 63.75 cm
Environmental Requirements | Pending
Ambient operating temperature | Long term: 41° to 104° F (5° to 40° C) Short term: 23° to 122° F (–5° ˚ to 50° C)
Ambient operating humidity | Long term: 5% to 85% (noncondensing) Short term: 5% to 95% (noncondensing)
Ambient storage temperature | –40° ˚ to 158° F (–40° ˚ to 70° C), 95% relative humidity
Ambient storage humidity | 5% to 95% (noncondensing)
Heat Dissipation | 1920 W, 6553 BTU/hour maximum
DC Input |
Voltage | –40 to –72 VDC NOTE: If the voltage rises above –40 VDC, the system powers off. The system does not power on again until the input voltage reaches –43 +/– 0.5 VDC.
Current | 40 A @ –48 VDC
Power | 1920 W
Redundancy (input power) | 2 independent line feeds
Space Requirements | 3 feet (90 cm) behind router or rack Do not block air vents on sides of the router Do not place equipment that exhausts hot air to left on the right of the router.
Airflow | Air intake occurs from the right side of the router. Air is exhausted out of the left side of the router.
NEBS Certification Level 3 | Pending
Safety Agency Certification | AS/NZS 60950:2000 Safety of Information Technology Equipment CAN/CSA-C22.2, No. 60950-1–03, First Edition, Information Technology Equipment - Safety - Part 1: General Requirements EN60825-1, Safety of Laser Products - Part 1: Equipment Class, Requirements, and User's Guide (2001) EN 60950-1:2001, First Edition, Information Technology Equipment - Safety - Part 1: General Requirements IEC 60950-1(2001-10) Ed. 1.0 Information Technology Equipment - Safety - Part 1: General Requirements Low Voltage Directive (73/23/EEC) UL 60950-1, First Edition, Information Technology Equipment - Safety - Part 1: General Requirements
Electromagnetic Emissions Agency Certification | AS/NZS CISPR 22:2004 EMC Directive (89/336/EEC) EN 300 132–2 (Narrowband and Wideband) EN55022 Class A (CISPR-22 Class A) EN55024, Annex C for WAN Equipment Performance Criteria A, B, and C EN 61000-4-2, EN 61000-4-3, EN 61000-4-4, EN 61000-4-6 ETSI 300-386, Telecommunication Network Equipment; ElectroMagnetic Compatibility (EMC) requirements FCC Part 15 Class A IECS-03 Issue 3 Class A VCCI (Voluntary Control Council for Interference by Information Technology Equipment)

[Contents] [Prev] [Next] [Index] [Report an Error]