[Contents] [Prev] [Next] [Index] [Report an Error]

# set priority

#### Syntax

set priority priorityValue

no set priority

#### Release Information

Command introduced in JUNOSe Release 8.2.0.

#### Description

Configures a priority value for the <S, G>data stream. Dynamic multicast admission control enables only prioritized groups to join the interface after the configured priority limit is reached on the physical port. The system records the priority when a new <S, G> entry is created. The no version removes the priority value.

#### Options

- priorityValue—Priority value for the <S, G> data stream; the default is 0

#### Mode

Route Map Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]