[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring VPLS-Specific Settings

Purpose

To display information about all VPLS instances configured on the router:

Action

To display detailed information about all VPLS instances configured on the router:

    host1:ce3#show vpls connections

      BridgeGroup: vpls1(vpls)

        SiteName:               bangalore
        SiteId:                 1
        Transport Virtual Rtr:  pe1
        Multihomed priority:    200

    Connections status code:
    UP = Operational
    SC = Local and Remote Site Identifier Collision
    EM = Encapsulation Mismatch
    OR = Out of Range
    DN = VC Down because Remote PE Unreachable
    LD = Local Site Down
    RD = Remote Site Down
    AS = Max BGP AS path length exceeded
    OL = No Out Label
    LN = Local Site not Designated
    RN = Remote Site not Designated

    Site   State     Remote PE     In-label  Out-label  MPLS NH Idx  Up-down Time
    -----  -----  ---------------  --------  ---------  -----------  ------------
    2      UP     3.3.3.3          17        36         79           00:04:09
    3      UP     5.5.5.5          18        56         54           00:04:09

    host1# show vpls connections details
      BridgeGroup: vpls1(vpls)
            Bridge Mode:            default
            Aging Time:             300 secs
            Learning:               Enabled
            Max Learn:              Unlimited
            Link Status Snmp Traps: Disabled
            Subscriber Policy:      default Subscriber
            Port Count:             2
            Interface Count:        1
            Transport Virtual Rtr:  pe1
              Route Distinguisher:    1.1.1.1:10
            SiteName:               westford
            SiteId:                 1
            SiteRange:              10
            VPLS Route Targets
              Route Target: RT:100:1 (both)
            Flood Next Hop: Index 1048577
              MPLS next-hop: 20, label 46, resolved by MPLS next-hop 19
                MPLS next-hop: 19, resolved by MPLS next-hop 17, peer 2.2.2.2
                  MPLS next-hop: 17, label 82 on ATM2/0.10, nbr 10.10.10.2
            Interface            Port       Status
    -------------------------   ------   ------------
    FastEthernet3/1             1        Up
    vpls vpls1                  2        Up
    Connections status code:
    UP = Operational
    SC = Local and Remote Site Identifier Collision
    EM = Encapsulation Mismatch
    OR = Out of Range
    DN = VC Down because Remote PE Unreachable
    LD = Local Site Down
    RD = Remote Site Down
    AS = Max BGP AS path length exceeded
    OL = No Out Label
    Site   State     Remote PE     In-label  Out-label  MPLS NH Idx  Up-down Time
    -----  -----  ---------------  --------  ---------  -----------  ------------
    2      UP     2.2.2.2          17        46         20           00:02:56
      BridgeGroup: vpls2(vpls)
            Bridge Mode:            default
            Aging Time:             300 secs
            Learning:               Enabled
            Max Learn:              Unlimited
            Link Status Snmp Traps: Disabled
            Subscriber Policy:      default Subscriber
            Port Count:             2
            Interface Count:        1
            Transport Virtual Rtr:  pe1
              Route Distinguisher:    1.1.1.1:10
            SiteName:               westford
            SiteId:                 1
            SiteRange:              20
            VPLS Route Targets
              Route Target: RT:100:2 (both)
            Flood Next Hop: Index 1048578
              MPLS next-hop: 21, label 56, resolved by MPLS next-hop 19
                MPLS next-hop: 19, resolved by MPLS next-hop 17, peer 2.2.2.2
                  MPLS next-hop: 17, label 82 on ATM2/0.10, nbr 10.10.10.2
            Interface            Port       Status
    -------------------------   ------   ------------
    ATM2/0.12                   1        Up
    vpls vpls2                  2        Up
    Connections status code:
    UP = Operational
    SC = Local and Remote Site Identifier Collision
    EM = Encapsulation Mismatch
    OR = Out of Range
    DN = VC Down because Remote PE Unreachable
    LD = Local Site Down
    RD = Remote Site Down
    AS = Max BGP AS path length exceeded
    OL = No Out Label
    Site   State     Remote PE     In-label  Out-label  MPLS NH Idx  Up-down Time
    -----  -----  ---------------  --------  ---------  -----------  ------------
    2      UP     2.2.2.2          27        56         21           00:02:56

Meaning

Table 98 lists the show vpls connections command output fields.

Table 98: show vpls connections Output Fields

Field Name | Field Description
--- | ---
BridgeGroup | Name of the VPLS instance for which information is displayed
Bridge Mode | Bridging capability currently enabled; for a VPLS instance, this field always displays default
Aging Time | Length of time, in seconds, that a MAC address entry can remain in the forwarding table before expiring
Learning | Whether acquisition of dynamically learned MAC addresses is enabled or disabled
Max Learn | Maximum number of dynamic MAC addresses that the VPLS instance can learn
Link Status Snmp Traps | Whether SNMP link status processing is enabled or disabled
Subscriber Policy | Name of the subscriber policy currently in effect
Port Count | Number of ports currently configured for the VPLS instance, including network interfaces and the VPLS virtual core interface
Interface Count | Number of network interfaces currently configured for the VPLS instance
Transport Virtual Rtr | Name of the transport virtual router configured for the VPLS instance
Route Distinguisher | Unique route distinguisher configured for the VPLS instance
SiteName | Site name configured for the VPLS instance
Transport Virtual Rtr | Identifier for the PE router that acts as the transport virtual router for the VPLS instance
Multihomed priority | Priority of the VPLS instance to serve as the backup PE router for the CE device in the event of a network failure in the multihomed configuration; indicates also that the site is multihomed
SiteId | Numerical site identifier configured for the VPLS instance
SiteRange | Maximum number of sites that can participate in the VPLS domain associated with the VPLS instance
VPLS Route Targets | Extended community identifiers, also known as route targets, for each VPLS instance configured on the router
Flood Next Hop | Index number of the MPLS next hop to which the router floods packets with unknown destination addresses. For more information about displaying MPLS next hops and any available next-hop statistics, see Monitoring MPLS Next Hops in Monitoring MPLS .
Interface | Type and specifier of the network interfaces and VPLS virtual core interface associated with the VPLS instance; vpls vplsName in this field identifies the VPLS virtual core interface
Port | Port number of the module on which the network interface or VPLS virtual core interface resides
Status | Operational status of the physical interface: Up, Down, LowerLayerDown, NotPresent
Connections status code | Possible status codes for the VPLS connection that appear in the State field
Site | Remote site identifier
State | Status of the connection with the remote VPLS instance; possible values for this field appear in the Connections status code legend in the command display
Remote PE | IP address of the remote VPLS edge (VE) router, which is analogous to the remote provider edge (PE) router in a BGP/MPLS VPN configuration
In-label | Incoming MPLS label from the remote site
Out-label | Outgoing MPLS label used to reach the remote site
MPLS NH Idx | MPLS next-hop index number that corresponds to the outgoing MPLS label
Up-down Time | Time since the last state change for this VPLS connection

#### Related Topics

- show vpls connections

[Contents] [Prev] [Next] [Index] [Report an Error]