[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls traffic-eng link-management timers periodic-flooding

#### Syntax

mpls traffic-eng link-management timers periodic-flooding frequency

no mpls traffic-eng link-management timers periodic-flooding

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the interval at which bandwidth values are flooded to the entire network. Configuring a value of 0 turns off flooding. The no version restores the default value, 180.

#### Options

- frequency—Interval in seconds, a value in the range 0–3600

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]