> - Download PDFs
> - radius dynamic-request server
> - Related Topics
> - Configuring RADIUS-Based Mirroring

> # radius dynamic-request server

> #### Syntax

> [ no ] radius dynamic-request server ipAddress

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Specifies the IP address of a RADIUS dynamic-request server and puts the E-series router into RADIUS Configuration mode. The no version deletes the instance of the RADIUS server.

> | Note: The radius dynamic-request server command replaces the functionality of the radius disconnect client command. The RADIUS Disconnect Configuration mode is deprecated. Use the radius dynamic-request server command to enter RADIUS Configuration mode and configure options formerly available in RADIUS Disconnect Configuration mode.

> #### Options

> - ipAddress—IP address of the server

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.