[Contents] [Prev] [Next] [Index] [Report an Error]

# show qos interface-hierarchy

#### Syntax

To display the interface hierarchy for interfaces:

show qos interface-hierarchy interface interfaceType interfaceSpecifier [ atmVpi | s-vlanIdValue ] [ filter ]

To display the interface hierarchy for L2TP sessions:

show qos interface-hierarchy l2tp session sessionName [ filter ]

To display the interface hierarchy for tunnel-service interfaces:

show qos interface-hierarchy tunnel-server interfaceSpecifier [ filter ]

To display the interface hierarchy for an interface set:

show qos interface-hierarchy qos-interface-set interfaceSetName [ filter ]

To display the interface hierarchy for an interface superset:

show qos interface-hierarchy qos-interface-superset interfaceSupersetName [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
atmVpi and s-vlanIdValue variables added in JUNOSe Release 7.1.0.

qos-interface-set keyword and interfaceSetName variable added in JUNOSe Release 9.2.0.

qos-interface-superset keyword and interfaceSupersetName variable added in JUNOSe Release 9.2.0.

#### Description

Displays information about the router’s QoS interface hierarchy.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- atmVpi—Virtual path identifier of this PVC; number in the range 0–255
- s-vlanIdValue—S-VLAN ID number in the range 0–4095
- sessionName —Name of the L2TP session
- interfaceSupersetName—Name of the interface superset
- interfaceSetName—Name of the interface set
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Monitoring the QoS Profiles Attached to an Interface

[Contents] [Prev] [Next] [Index] [Report an Error]