[Contents] [Prev] [Next] [Index] [Report an Error]

# Subscriber Interfaces Platform Considerations

For information about modules that support subscriber interfaces on the ERX-7xx models, ERX-14xx models, and the ERX-310 router:

- See ERX Module Guide, Table 1, ERX Module Combinations for detailed module specifications.
- See ERX Module Guide, Appendix A, Module Protocol Support for information about the modules that support subscriber interfaces.

For information about modules that support subscriber interfaces on the E120 router and the E320 router:

- See E120 and E320 Module Guide, Table 1, Modules and IOAs for detailed module specifications.
- See E120 and E320 Module Guide, Appendix A, IOA Protocol Support for information about the modules that support subscriber interfaces.

## Interface Specifiers

The configuration task examples in this chapter use the slot/port format to specify an interface. However, the interface specifier format that you use depends on the router that you are using.

For ERX-7xx models, ERX-14xx models, and ERX-310 routers, use the slot/port format. For example, the following command specifies a Gigabit Ethernet interface on slot 0, port 1 of an ERX-7xx model, ERX-14xx model, or ERX-310 router.

`

host1(config)#interface gigabitEthernet 0/1

`

For E120 and E320 routers, use the slot/adapter/port format, which includes an identifier for the bay in which the I/O adapter (IOA) resides. In the software, adapter 0 identifies the right IOA bay (E120 router) and the upper IOA bay (E320 router); adapter 1 identifies the left IOA bay (E120 router) and the lower IOA bay (E320 router). For example, the following command specifies a Gigabit Ethernet interface on slot 5, adapter 0, port 0 of an E320 router.

`

host1(config)#interface gigabitEthernet 5/0/0

`

For more information about supported interface types and specifiers on E-series routers, see Interface Types and Specifiers JUNOSe Command Reference Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]