[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Router to Start Mirroring When User Logs On

To configure the router to support user-initiated mirroring, which starts when the user logs in:

1. Configure RADIUS server authentication information in the router. See JUNOSe Broadband Access Configuration Guide for information.
2. Configure the analyzer interface to send the mirrored traffic to the analyzer device.
   `
   host1(config)#interface fastEthernet 4/0
   host1(config-if)#ip analyzer
   `

   Alternatively, for increased security, create the analyzer interface at one end of an IPSec tunnel to the analyzer device.

   `
   host1(config)# interface tunnel ipsec:mirror3 transport-virtual-router default
   host1(config-if)#ip analyzer
   host1(config-if)#exit
   host1(config)#ip route 192.168.99.2 255.255.255.255 tunnel ipsec:mirror3
   `

[Contents] [Prev] [Next] [Index] [Report an Error]