[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 pim rp-address

#### Syntax

[ no ] ipv6 pim rp-address ipv6Address [ ipv6AccessList ] [ override ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies a static PIM group–to–RP mapping. The no version clears the mapping from this interface.

#### Options

- ipv6Address—IPv6 address of the router you want to designate as an RP router
- ipv6AccessList—Name of the IPv6 access list that specifies which multicast groups use this RP
- override—Specifies that this static RP mapping has priority over group-to-RP mappings learned by auto-RP

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]