[Contents] [Prev] [Next] [Index] [Report an Error]

# pos scramble-atm

#### Syntax

[ no ] pos scramble-atm

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables payload scrambling on a POS interface. When enabled, both sides of the connection must be using the scrambling algorithm. The router uses a 43rd-order synchronous scrambler to scramble the output data. Scrambling is enabled by default. The no version disables scrambling on the POS interface.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]