[Contents] [Prev] [Next] [Index] [Report an Error]

# Managing Virtual Routers

Your router supports SNMP management of virtual routers. This support is based on an SNMP community string proxy to select particular instances of virtual routers. The entity MIB is used to model the physical container to the logical relationship of the virtual router implementation. See Configuring Virtual Routers.

[Contents] [Prev] [Next] [Index] [Report an Error]