> - Download PDFs
> - vlan classifier-list
> - Related Topics
> - Creating or Modifying Classifier Control Lists for VLAN Policy Lists

> # vlan classifier-list

> #### Syntax

> vlan classifier-list classifierName
> [ traffic-class className ] [ color { green | yellow | red } ]
> [ user-packet-class userPacketClassValue ] [ user-priority userPriorityValue ]

> no vlan classifier-list classifierName [ classifierNumber ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Creates or modifies a VLAN classifier control list. The no version deletes the classifier control list.

> #### Options

> - classifierName—Name of a classifier list entry
> - className—Name of a traffic class; the router supports up to eight traffic classes
> - green—Matches packet color to green, indicating a low drop preference
> - yellow—Matches packet color to yellow, indicating a medium drop preference
> - red—Matches packet color to red, indicating a high drop preference
> - userPacketClassValue—Value of the user packet class in the range 0–15
> - userPriorityValue—Value of the user priority bits in the range 0–7
> - classifierNumber—Index of the classifier control list entry to be deleted; an integer in the range 1–10000

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.