[Contents] [Prev] [Next] [Index] [Report an Error]

# Before You Configure IPv6

Before you configure IPv6, you must create the lower-layer interfaces over which IPv6 traffic flows. In this release, the following modules support IPv6 configuration:

- ATM OC3/STM-1
- ATM OC12/STM-4
- Fast Ethernet (FE-8)
- Gigabit Ethernet (GE)
- 10-Gigabit Ethernet (10GE)
- OC48 POS (PPP only)

For example, to configure an ATM interface:

`

host1(config)#interface atm 1/0
host1(config-if)#atm sonet stm-1
host1(config-if)#no loopback
host1(config-if)#atm clock internal chassis
host1(config-if)#interface atm 1/0.10
host1(config-if)#atm pvc 10 0 20 aal5snap

`

See JUNOSe Link Layer Configuration Guide for information about configuring an ATM interface. See JUNOSe Physical Layer Configuration Guide for information about configuring an Ethernet interface.

[Contents] [Prev] [Next] [Index] [Report an Error]