[Contents] [Prev] [Next] [Index] [Report an Error]

# lsp-refresh-interval

#### Syntax

lsp-refresh-interval seconds

no lsp-refresh-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the link-state packet rate at which locally generated IS-IS link-state packets are periodically transmitted. The no version restores the default value, 900.

#### Options

- seconds—Number in the range 1–65535; the refresh interval in seconds; default value is 900

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]