[Contents] [Prev] [Next] [Index] [Report an Error]

# network area

#### Syntax

[ no ] network ipNet maskWildCard area { areaId | areaIdInt }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Defines the interfaces on which OSPF runs and the area ID for those interfaces. The no version deletes OSPF interfaces, ranges, and areas.

| Note: Before you issue this command, you must first configure one or more interfaces with an IP address that is within the range specified by ipNet. Create address ranges that do not overlap; you can attach only the same range of interfaces to a single area.

#### Options

- ipNet—Network number
- maskWildCard—Wild-card mask for the network number
- areaId—OSPF area ID in IP address format
- areaIdInt—OSPF area ID as a decimal value, in the range 0–4294967295

#### Mode

Router Configuration

#### Related Topics

- Configuring Routing in the Core Network for VPLS in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]