[Contents] [Prev] [Next] [Index] [Report an Error]

# frame-relay classifier-list

#### Syntax

frame-relay classifier-list classifierName [ traffic-class trafficClassName ]
[ color { green | yellow | red } ] [ user-packet-class userPacketClassValue ]
[ de-bit deValue ]

no frame-relay classifier-list classifierName [ classifierNumber ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Creates or modifies a Frame Relay classifier control list. The no version removes the classifier control list.

#### Options

- classifierName—Name of the classifier control list entry
- trafficClassName—Name of the traffic class to match
- green—Matches packet color to green, indicating a low drop preference
- yellow—Matches packet color to yellow, indicating a medium drop preference
- red—Matches packet color to red, indicating a high drop preference
- userPacketClassValue—User packet value to match in the range 0–15
- deValue—Value of the DE bit to match; 0 or 1

#### Mode

Global Configuration

#### Related Topics

- Creating or Modifying Classifier Control Lists for Frame-Relay Policy Lists

[Contents] [Prev] [Next] [Index] [Report an Error]