[Contents] [Prev] [Next] [Index] [Report an Error]

# color-mark-profile

#### Syntax

[ no ] [ ip | ipv6 | mpls ] color-mark-profile profileName

#### Release Information

Command introduced in JUNOSe Release 7.2.0.

#### Description

Translates the packet color (independent of its type) to a type-dependent mark (for ToS or EXP), which is applied to a packet after it has exited a rate-limit hierarchy. If translation is not configured for a color, then packets of that color are not changed. The no version deletes the color-mark profile.

#### Options

- profileName—Name of the rate-limit profile to be used in a policy (up to 40 alphanumeric characters)

#### Mode

Color Mark Profile Configuration, Global Configuration

#### Related Topics

- Hierarchical Rate Limits Overview
- Policy Rule Precedence

[Contents] [Prev] [Next] [Index] [Report an Error]