> - Download PDFs
> - snmp-server enable traps
> - Related Topics
> - Monitoring SNMP Secure Packet Mirroring Traps

> # snmp-server enable traps

> #### Syntax

> To enable and configure trap severity level on a global basis:

> [ no ] snmp-server enable traps [ trapCategory | snmp authentication ]
> [ trapfilters trapFilter ]

> To specify the trap severity level on a per-category basis:

> snmp-server enable traps { trapCategory | snmp authentication } per-category-trapFilters trapFilter

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> ip keyword added in JUNOSe Release 7.1.0.
> packetMirror keyword added in JUNOSe Release 7.2.0.
> per-category-trapFilters keyword added in JUNOSe Release 9.3.0.

> #### Description

> Enables and configures global and category-level SNMP trap generation. The no version disables SNMP trap generation globally. There is no no version for the command to specify the trap severity level on a per-category basis.

> #### Options

> - trapCategory—SNMP trap category
>   - addrPool—Local address pool traps
>   - atmPing—E-series router proprietary ATM ping traps
>   - bfdmib—BFD MIB traps
>   - bgp—BGP state change traps
>   - bulkstats—Bulkstats file full and nearly full traps
>   - cliSecurityAlert—Security alerts traps
>   - dhcp—DHCP traps
>   - dismanEvent—Distributed management (disman) event traps
>   - dosProtectionPlatform—DoS protection platform traps
>   - dvmrp—DVMRP traps
>   - dvmrpProp—E-series router proprietary DVMRP traps
>   - environment—Power, temperature, fan, and memory utilization traps
>   - fileXfer—File transfer status change traps
>   - haRedundancy—High availability and redundancy traps
>   - inventory—Router inventory and status traps
>   - ip—Internet Protocol traps
>   - ldp—LDP traps
>   - link—SNMP linkUp and linkDown traps
>   - log—System log capacity traps
>   - mobileIpv4—Mobile IPv4 traps
>   - mplste—Mplste traps
>   - mrouter—Mrouter traps
>   - ntp—E-series router proprietary traps
>   - ospf—OSPF traps
>   - packetMirror—Secure packet mirroring traps; visible only if packet mirroring is enabled
>   - pim—PIM traps
>   - ping—Ping operation traps (in disman remops MIB)
>   - radius—RADIUS authentication and authorization servers
>   - routeTable—Maximum route limit and warning threshold traps; when this trap is generated, the actual value of the exceeded warning threshold is displayed
>   - sonet—SONET traps
>   - snmp—SNMP coldStart, warmStart, link, and authenticationFailure traps
>   - traceroute—Traceroute operation traps (in disman remops MIB)
>   - vrrp—VRRP traps
> - snmp—Specifies the SNMP coldStart, warmStart, and authenticationFailure traps
> - authentication—Specifies the SNMP authenticationFailure trap
> - trapFilters—Specifies the trap severity level at a global level; if the per-category trap severity level is not set for a particular category, this setting is applied to that category
> - trapFilter—Minimum severity level for filtering traps at a global level or for a specified category
>   - emergency—Severity level 0
>   - alert—Severity level 1
>   - critical—Severity level 2
>   - error—Severity level 3
>   - warning—Severity level 4
>   - notice—Severity level 5
>   - informational—Severity level 6
>   - debug—Severity level 7
> - per-category-trapFilters—Specifies the trap severity level for a particular category; this setting overrides the severity level set at the global level for this category
> - trapFilter—Minimum severity level for filtering traps for the specified category

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.