> - Download PDFs
> - mirror disable
> - Related Topics
> - Configuring CLI-Based Mirroring
> - Configuring RADIUS-Based Mirroring

> # mirror disable

> #### Syntax

> mirror disable triggerType triggerValue

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> nas-port-id added in JUNOSe Release 7.1.0.

> #### Description

> Disables a packet mirroring session that was dynamically configured for a subscriber; uses the trigger information to identify the subscriber's session. There is no no version.

> #### Options

> - triggerType—One of the following RADIUS attributes that was used as the trigger to start the packet mirroring session
>   - acct-session-id—Acct-Session-Id, RADIUS attribute [44]
>   - calling-station-id—Calling-Station-Id, RADIUS attribute [31]
>   - ip-address—Framed-IP-Address, RADIUS attribute [8]; associated with the virtual router where the command is issued, RADIUS VSA [26-1]
>   - nas-port-id—NAS-Port-Id, RADIUS attribute [87]
>   - username—User-Name, RADIUS attribute [1]; associated with the virtual router where the command is issued, RADIUS VSA [26-1]
> - triggerValue—Value of the triggerType (the specified RADIUS attribute) that identifies the subscriber

> #### Mode

> Privileged Exec

> #### Updated: 2009-04-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.