[Contents] [Prev] [Next] [Index] [Report an Error]

# aggregation-node

#### Syntax

aggregation-node { nodeValue | atm | atm-vc | atm-vp vpValue | ethernet | fr-vc |
forwarding | svlan svlanValue | vlan }

no aggregation-node

#### Release Information

Command introduced in JUNOSe Release 8.0.0.

#### Description

Configures the aggregation node value. The no version restores the default value, where the forwarding interface becomes the aggregation node.

#### Options

- nodeValue— Aggregation node number in the range 1–65535
- vpValue—ATM VPI number in the range 0–255
- svlanValue—SVLAN ID number in the range 0–4095

#### Mode

Policy Parameter Configuration

#### Related Topics

- Creating a Classifier Group for a Policy List

[Contents] [Prev] [Next] [Index] [Report an Error]