[Contents] [Prev] [Next] [Index] [Report an Error]

# atm atm1483 advisory-rx-speed

#### Syntax

atm atm1483 advisory-rx-speed speed

no atm atm1483 advisory-rx-speed

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets an advisory receive (RX) speed that the LAC sends in the RX Connect-Speed AVP [38] to the LNS. The no version restores the default behavior, in which the RX speed is not sent to the LNS.

#### Options

- speed—Speed in the range 0–2147483647 kbps

#### Mode

Profile Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]