[Contents] [Prev] [Next] [Index] [Report an Error]

# Setting a Baseline for VPLS Statistics

You can use the following baseline commands to set a statistics baseline for a VPLS instance, for a network interface associated with a VPLS instance, or for the VPLS virtual core interface associated with a VPLS instance. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved.

Use the delta keyword with the show bridge commands display baselined statistics.

Tasks to set a baseline for VPLS statistics are:

- Setting a Baseline for a VPLS Instance
- Setting a Baseline for a Network Interface Associated with a VPLS Instance
- Setting a Baseline for the VPLS Virtual Core Interface Associated with a VPLS Instance

## Setting a Baseline for a VPLS Instance

To set a statistics baseline for a VPLS instance:

- Issue the baseline bridge command.
  `
  host1#baseline bridge vplsA
  `

There is no no version.

## Setting a Baseline for a Network Interface Associated with a VPLS Instance

To set a statistics baseline for the VPLS network interface:

- Issue the baseline bridge interface command.
  `
  host1#baseline bridge interface gigabitEthernet 4/1
  `

## Setting a Baseline for the VPLS Virtual Core Interface Associated with a VPLS Instance

To set a statistics baseline for the VPLS virtual core interface:

- Issue the baseline bridge interface vpls command.
  `
  host1#baseline bridge interface vpls vplsA
  `

There is no no version.

#### Related Topics

- baseline bridge
- baseline bridge interface
- baseline bridge interface vpls

[Contents] [Prev] [Next] [Index] [Report an Error]