[Contents] [Prev] [Next] [Index] [Report an Error]

## Example: Port-Type QoS Profile Attachment

In this example, three ATM subinterfaces are configured on an ATM port:

- ATM 11/0.1—QoS profile qp1 is attached
- ATM 11/0.2—QoS profile qp2 is attached
- ATM 11/0.3—No QoS profile is attached

The major ATM interface, 11/0, does not have a QoS profile explicitly attached. Therefore, by default the atm-default QoS port-type profile is attached.

Figure 37: Attaching QoS Profiles to ATM Subinterfaces

To configure this example:

1. Create and configure QoS profile qp1.
   `
   host1(config)#qos-profile qp-1
   host1(config-qos-profile)#atm-vp node scheduler-profile sp1
   host1(config-qos-profile)#atm-vc queue traffic-class tc1 scheduler-profile sp1 queue-profile qp1
   host1(config-qos-profile)#atm-vc queue traffic-class tc2 scheduler-profile sp2 queue-profile qp2
   host1(config-qos-profile)#atm-vc queue traffic-class tc3 scheduler-profile sp3 queue-profile qp3
   host1(config-qos-profile)#atm-vc queue traffic-class tc4 scheduler-profile sp4 queue-profile qp4
   host1(config-qos-profile)#atm-vc queue traffic-class tc5 scheduler-profile sp5 queue-profile qp5
   host1(config-qos-profile)#exit
   `
2. Create and configure QoS profile qp2.
   `
   host1(config)#qos-profile qp2
   host1(config-qos-profile)#atm-vp node scheduler-profile sp1
   host1(config-qos-profile)#atm-vc queue traffic-class tc1 scheduler-profile sp1 queue-profile qp1
   host1(config-qos-profile)#atm-vc queue traffic-class tc2 scheduler-profile sp2 queue-profile qp2
   host1(config-qos-profile)#atm-vc queue traffic-class tc3 scheduler-profile sp3 queue-profile qp3
   host1(config-qos-profile)#exit
   `
3. Attach the QoS profiles to the ATM subinterfaces, as shown in Figure 37.
   `
   host1(config)#interface atm 11/0.1
   host1(config-subif)#qos-profile qp1
   host1(config-subif)#exit
   host1(config)#interface atm 11/0.2
   host1(config-subif)#qos-profile qp2
   host1(config-subif)#exit
   `
4. Display the QoS interface hierarchy for ATM interface 11/0. This display shows all QoS attachments above interface 11/0.

   If no QoS profiles are attached above the specified interface, the router shows the first attachment below the specified interface.

       host1# show qos interface-hierarchy interface atm 11/0
       attachment@ atm-vc ATM11/0.2:
           qos          interface  rule  traffic       scheduler  queue  t-class
       profile           type      type  class         profile   profile  group
       -------          ---------  ----  -------       --------- ------- -------
       qp2@ATM11/0.2    atm-vp     node                sp1       default
       qp2@ATM11/0.2    atm-vc     queue tc1           sp1       qp1
       qp2@ATM11/0.2    atm-vc     queue tc2           sp2       qp2
       qp2@ATM11/0.2    atm-vc     queue tc3           sp3       qp3
       atm-default @atm ip         node                default   default
       atm-default @atm atm-vc     node                default   default
       atm-default @atm Bridge     node                default   default
       atm-default @atm ipv6       node                default   default
       atm-default @atm ip         queue  best-effort  default   default
       atm-default @atm atm        queue  best-effort  default   default
       atm-default @atm atm-vc     queue  best-effort  default   default
       atm-default @atm Bridge     queue  best-effort  default   default
       atm-default @atm ipv6       queue  best-effort  default   default
       attachment@ atm-vc ATM11/0.1:
           qos          interface  rule  traffic        scheduler  queue   t-class
       profile           type      type  class          profile    profile group
       -------          ---------  ----  -------        ---------  ------- -------
       qp1@ATM11/0.1    atm-vp     node                 sp1        default
       qp1@ATM11/0.1    atm-vc     queue   tc1          sp1        qp1
       qp1@ATM11/0.1    atm-vc     queue   tc2          sp2        qp2
       qp1@ATM11/0.1    atm-vc     queue   tc3          sp3        qp3
       qp1@ATM11/0.1    atm-vc     queue   tc4          sp4        qp4
       qp1@ATM11/0.1    atm-vc     queue   tc5          sp5        qp5
       atm-default @atm ip         node                 default    default
       atm-default @atm atm-vc     node                 default    default
       atm-default @atm Bridge     node                 default    default
       atm-default @atm ipv6       node                 default    default
       atm-default @atm ip         queue   best-effort  default    default
       atm-default @atm atm        queue   best-effort  default    default
       atm-default @atm atm-vc     queue   best-effort  default    default
       atm-default @atm Bridge     queue   best-effort  default    default
       atm-default @atm ipv6       queue   best-effort  default    default

ATM subinterface 11/0.3 was not shown because no QoS profile is attached to it. You can display the QoS interface hierarchy for subinterface 11/0.3 by specifying the subinterface, as shown below. In this case, the QoS port-type profile, atm-default, is attached (by default) to the ATM major interface, ATM 11/0, below ATM subinterface 11/0.3. Because no QoS profile is attached to this ATM subinterface, the QoS port-type profile is applied.

The @atm in the qos profile column indicates that the row comes from a default QoS port-type profile that is below the interfaces shown: subinterfaces ATM 11/0.2 and ATM 11/0.1 in this example.

You can explicitly show the ATM subinterface that has no explicit QoS profile attachment, as shown below. In this case, attachment@ indicates the ATM major interface (11/0) below the subinterface.

    host1# show qos interface-hierarchy interface atm 11/0.3
    attachment@ atm ATM11/0:
        qos          interface  rule  traffic       scheduler  queue  t-class
    profile           type      type  class         profile   profile  group
    -------          ---------  ----  -------       --------- ------- -------
    atm-default@atm  ip         node                default   default
    atm-default@atm  atm-vc     node                default   default
    atm-default@atm  Bridge     node                default   default
    atm-default@atm  ipv6       node                default   default
    atm-default@atm  ip         queue best-effort   default   default
    atm-default@atm  atm        queue best-effort   default   default
    atm-default@atm  atm-vc     queue best-effort   default   default
    atm-default@atm  Bridge     queue best-effort   default   default
    atm-default@atm  ipv6       queue best-effort   default   default

[Contents] [Prev] [Next] [Index] [Report an Error]