[Contents] [Prev] [Next] [Index] [Report an Error]

# l2tp retransmission

#### Syntax

l2tp retransmission retries [ established | not-established ]

no l2tp retransmission [ retries ] [ established | not-established ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the number of retransmission retries, and allows you to apply the retry count to established and/or unestablished tunnels. If you do not include a keyword, the router applies the retry count to all tunnels. The no version resets the number of retransmissions to the default value, 5.

#### Options

- retries—Number in the range 2–10
- established—Applies the retry count only to established tunnels
- not-established—Applies the retry count only to tunnels that are not established

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]