[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 access-list

#### Syntax

Extended IPv6 access list:

ipv6 access-list accessListName { permit | deny } { srcIPv6Prefix |
host srcIPHost | any } { dstIPv6Prefix | host dstIPHost | any } [ log ]

no ipv6 access-list accessListName [ { permit | deny } { srcIPv6Prefix |
host srcIPv6Host | any } { dstIPv6Prefix | host dstIPv6Host | any } [ log ] ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Defines an IPv6 access list. The extended access list enables you to specify a destination address or host, precedence, and type of service. Imposes an implicit last rule of “ deny ip any any” to deny all routes that do not match previous rules in the access list. The no version removes the IPv6 access list, the specified entry in an access list, or the log for a specified entry.

#### Options

- accessListName—String of up to 32 alphanumeric characters
- permit—Permits access if the conditions are matched
- deny—Denies access if the conditions are matched
- srcIPv6Prefix—Source IPv6 address and mask length from which the packet is being sent
- srcIPv6Host—Source host IPv6 address; assumes a mask length of 128
- any—Creates an address of :: with a mask length of 0
- dstIPv6Prefix—Destination IP address and mask length
- dstIPv6Host—Destination host IPv6 address to which the packet is being sent
- log—Logs an Info event into the ipAccessList log whenever the access-list rule is matched

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]