[Contents] [Prev] [Next] [Index] [Report an Error]

# l2tp destination lockout-timeout

#### Syntax

l2tp destination lockout-timeout timeOutValue

no l2tp destination lockout-timeout

#### Release Information

Command introduced in JUNOSe Release 7.2.0.

#### Description

Specifies the amount of time an L2TP destination remains in the lockout state after the destination becomes unavailable. When the timeout period expires, the router either begins the lockout test procedure (if configured to do so) or immediately returns the destination to service. The no version restores the default lockout timeout value.

#### Options

- timeOutValue—Number of seconds in the range 60–3600; default is 300 seconds (5 minutes)

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]