[Contents] [Prev] [Next] [Index] [Report an Error]

## Managing System Resources for Shadow Nodes

Each ASIC hardware type provides different node and queue resources.

Level 1 queues stack directly above the port; level 2 queues stack above a node and the port. The router implicitly creates the level 1 and level 2 queues.

Shadow node queues stack above a port node, a level 1 node, and a shadow node. Therefore, the shadow node queue is at level 3. The router does not implicitly create any nodes for the queues.

You can configure 64,000 level 1 queues using shadow nodes by specifying the group and shadow node rules in the QoS profile. Each level 1 queue is stacked above the port, the group node, and the shadow node; therefore, it requires 64,002 descriptors.

Table 15 lists the number of nodes required to create a queue.

Table 15: Shadow Node Consumption of Node and Queue Resources

| Level 1 Queues (at Port) | Level 2 Queues (at Node) | Shadow Node Queue
--- | --- | --- | ---
Required Nodes | 3 | 2 | 1

#### Related Topics

- Managing System Resources for Nodes and Queues
- Scaling Subscribers on the TFA ASIC with QoS

[Contents] [Prev] [Next] [Index] [Report an Error]