[Contents] [Prev] [Next] [Index] [Report an Error]

# Before You Configure VPLS

The JUNOSe implementation of VPLS uses features of transparent bridging, BGP, MPLS, LDP, BGP/MPLS VPNs, and layer 2 services over MPLS. We recommend that you have a thorough understanding of these protocols before you configure and use VPLS in your network.

#### Related Topics

- For more information about configuring transparent bridging, see the JUNOSe Link Layer Configuration Guide
- For more information about configuring the layer 2 interfaces that support VPLS, see the JUNOSe Physical Layer Configuration Guide and the JUNOSe Link Layer Configuration Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]