[Contents] [Prev] [Next] [Index] [Report an Error]

# bridge vpls route-target

#### Syntax

[ no ] bridge vplsName vpls route-target { import | export | both } extendedCommunity

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Creates or adds to a list of VPN extended communities that the router uses to determine which routes are imported by a VPLS instance that uses BGP as the signaling protocol. The no version removes a route target from the specified list.

A route is imported into the BGP address family for a specified VPLS instance when both of the following conditions are met:

- An update message with a route-target export list advertises a route.
- That list contains at least one route target that matches a route target in the route-target import list associated with a VPLS instance.

The bridge vpls route-target command is not valid for a VPLS instance that uses LDP as the signaling protocol. To configure a VPLS instance with LDP signaling, use the mpls ldp vpls vpls-id command and the mpls ldp vpls neighbor command.

| Note: The bridge vpls route-target command is available for a VPLS instance only after you issue the bridge vpls transport-virtual-router command, which creates the VPLS instance and configures the transport virtual router.

#### Options

- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command
- import—Adds the route target to the specified VPLS instance's import list; the VPLS instance accepts only routes that have at least one route target that matches a route target in the import list
- export—Adds the route target to the specified VPLS instance's export list; all routes advertised from this VPLS instance are associated with the export list
- both—Adds the route target to both the import list and export list of the specified VPLS instance. This is the recommended setting for a VPLS instance
- extendedCommunity—Two-part number in the format number1:number2 that identifies an extended community of VPNs, where:
  - number1—Autonomous system (AS) number or an IP address
  - number2—Unique integer; 32 bits if number1 is an AS number; 16 bits if number1 is an IP address

#### Mode

Global Configuration

#### Related Topics

- Configuring VPLS Instances with BGP Signaling in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]