[Contents] [Prev] [Next] [Index] [Report an Error]

# retransmit-interval

#### Syntax

retransmit-interval retransInterval

no retransmit-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the time between LSA retransmissions for the OSPF remote-neighbor interface when an acknowledgment for the LSA is not received. The no version restores the default value.

#### Options

- retransInterval—Number of seconds, in the range 0–3600; default value is 5

#### Mode

Remote Neighbor Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]