[Contents] [Prev] [Next] [Index] [Report an Error]

# broadcast

#### Syntax

broadcast { permit | deny }

no broadcast

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Modifies the subscriber policy for the broadcast protocol to define whether the subscriber (client) interfaces that belongs to a bridge group or to a VPLS instance forward (permit) or filter (deny) broadcast packets. The no version restores the default value, deny broadcast packets.

You cannot change the default subscriber policy values for trunk (server) interfaces that belongs to a bridge group or to a VPLS interface. You also cannot change the default subscriber policy values for a VPLS virtual core interface, which acts as a trunk interface. The VPLS virtual core interface represents all of the MPLS tunnels from the router to the remote VPLS edge (VE) device.

#### Options

- permit—Specifies that the subscriber interface associated with the bridge group or VPLS instance forwards broadcast packets
- deny—Specifies that the subscriber interface associated with the bridge group or VPLS instance filters broadcast packets

#### Mode

Subscriber Policy Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]