> - Download PDFs
> - remote host

> # remote host

> #### Syntax

> remote host { hostname | default }

> no remote host { hostname | default }

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Defines an L2TP host profile. Accesses the L2TP Destination Profile Host Configuration mode. The no version removes an L2TP host profile.

> #### Options

> - hostname—Name the LAC must supply in the hostname AVP of the receive SCCRQ; can be up to 64 characters in length (no spaces)
> - default—Allows the LAC to use any hostname in the hostname AVP

> #### Mode

> L2TP Destination Profile Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.